
FileVersion: 1

#######################
# Dates of last change
#######################

Date, 4pt measurement: 
Date, Horizontal tilt of bed: 
Date, Vertical tilt of bed: 

Date, Head 1, Intrinsic resolution: 
Date, Head 1, Collimator depth: 
Date, Head 1, Collimated beam: 
Date, Head 1, Aperture twist: 

Date, Head 2, Intrinsic resolution: 
Date, Head 2, Collimator depth: 
Date, Head 2, Collimated beam: 
Date, Head 2, Aperture twist: 

Date, Head 3, Intrinsic resolution: 
Date, Head 3, Collimator depth: 
Date, Head 3, Collimated beam: 
Date, Head 3, Aperture twist: 

Date, Head 4, Intrinsic resolution: 
Date, Head 4, Collimator depth: 
Date, Head 4, Collimated beam: 
Date, Head 4, Aperture twist: 


###########################
# Global system parameters
###########################

Standard image dimension: 256
Average pixel size [mm]: 1
Swap bytes? (no=0/yes=1): 0
Crystal thickness [mm]: 6.5
Pixel size at 128/1 [mm]: 2
Horizontal animal bed offset [mm]: 0
Horizontal tilt of animal bed [deg]: 0
Vertical tilt of animal bed [deg]: 0
Vertical animal bed offset [mm]: 0
Axial animal bed offset [mm]: 0
Diameter of pinhole [mm]: 1.5
Diameter of collimated source [mm]: 0.8
Length of collimated source [mm] 54
Number of detectors: 4
Quality of calibration [a.u.]: 0


###############################
# Detector specific parameters
###############################

Head 1, Collimator depth [mm]: 132.1
Head 1, Transaxial aperture offset [mm]: 0
Head 1, Axial aperture offset [mm]: 0
Head 1, Transaxial detector offset [mm]: 0
Head 1, Axial detector offset [mm]: 0
Head 1, Radius of rotation [mm]: 44.9
Head 1, Displayed radius [mm]: 0
Head 1, Radius offset [mm]: 0
Head 1, Collimated beam, Y [mm]: 0
Head 1, Collimated beam, Z [mm]: 0
Head 1, Intrinsic resolution [mm]: 2.1
Head 1, Pixel size [mm]: 1.003
Head 1, Aperture twist [deg]: 0
Head 1, Twist of image matrix [deg]: 0
Head 1, Transaxial flip (no=0/yes=1): 1
Head 1, Axial flip (no=0/yes=1): 0
Head 1, Quality of linearity [a.u.]: 0

Head 2, Collimator depth [mm]: 132.1
Head 2, Transaxial aperture offset [mm]: 0
Head 2, Axial aperture offset [mm]: 0
Head 2, Transaxial detector offset [mm]: 0
Head 2, Axial detector offset [mm]: 0
Head 2, Radius of rotation [mm]: 44.9
Head 2, Displayed radius [mm]: 0
Head 2, Radius offset [mm]: 0
Head 2, Collimated beam, Y [mm]: 0
Head 2, Collimated beam, Z [mm]: 0
Head 2, Intrinsic resolution [mm]: 2.1
Head 2, Pixel size [mm]: 1.003
Head 2, Aperture twist [deg]: 0
Head 2, Twist of image matrix [deg]: 0
Head 2, Transaxial flip (no=0/yes=1): 1
Head 2, Axial flip (no=0/yes=1): 0
Head 2, Quality of linearity [a.u.]: 0

Head 3, Collimator depth [mm]: 132.1
Head 3, Transaxial aperture offset [mm]: 0
Head 3, Axial aperture offset [mm]: 0
Head 3, Transaxial detector offset [mm]: 0
Head 3, Axial detector offset [mm]: 0
Head 3, Radius of rotation [mm]: 44.9
Head 3, Displayed radius [mm]: 0
Head 3, Radius offset [mm]: 0
Head 3, Collimated beam, Y [mm]: 0
Head 3, Collimated beam, Z [mm]: 0
Head 3, Intrinsic resolution [mm]: 2.1
Head 3, Pixel size [mm]: 1.003
Head 3, Aperture twist [deg]: 0
Head 3, Twist of image matrix [deg]: 0
Head 3, Transaxial flip (no=0/yes=1): 1
Head 3, Axial flip (no=0/yes=1): 0
Head 3, Quality of linearity [a.u.]: 0

Head 4, Collimator depth [mm]: 132.1
Head 4, Transaxial aperture offset [mm]: 0
Head 4, Axial aperture offset [mm]: 0
Head 4, Transaxial detector offset [mm]: 0
Head 4, Axial detector offset [mm]: 0
Head 4, Radius of rotation [mm]: 44.9
Head 4, Displayed radius [mm]: 0
Head 4, Radius offset [mm]: 0
Head 4, Collimated beam, Y [mm]: 0
Head 4, Collimated beam, Z [mm]: 0
Head 4, Intrinsic resolution [mm]: 2.1
Head 4, Pixel size [mm]: 1.003
Head 4, Aperture twist [deg]: 0
Head 4, Twist of image matrix [deg]: 0
Head 4, Transaxial flip (no=0/yes=1): 1
Head 4, Axial flip (no=0/yes=1): 0
Head 4, Quality of linearity [a.u.]: 0


######################################
# Phantom descriptor: Collimated beam
######################################

CollBeam, Hole diameter [mm]: 0.8
CollBeam, Collimation length [mm]: 54


#######################################
# Phantom descriptor: Positioning grid
#######################################

IntRes, Transaxial grid dimension: 4
IntRes, Axial grid dimension: 4
IntRes, Transaxial grid spacing [mm]: 50
IntRes, Axial grid spacing [mm]: 50
IntRes, CollBeam offset [mm]: 9
IntRes, Offset position index (0,1...): 5
IntRes, Transaxial position offset [mm]: -7


#######################################
# Phantom descriptor: Collimator depth
#######################################

Depth, Number of sources: 4
Depth, Phantom height [mm]: 64.5
Depth, Phantom asymmetry (hor=0/ver=1): 1

Depth 1, Y position [mm]: 25.0
Depth 1, Z position [mm]: 35.0
Depth 2, Y position [mm]: -25.0
Depth 2, Z position [mm]: 25.0
Depth 3, Y position [mm]: 25.0
Depth 3, Z position [mm]: -25.0
Depth 4, Y position [mm]: -25.0
Depth 4, Z position [mm]: -35.0


#####################################
# Phantom descriptor: Aperture twist
#####################################

Twist, Rear position, Y [mm]: 17.0
Twist, Rear position, Z [mm]: 17.0
Twist, Front position, Y [mm]: -17.0
Twist, Front position, Z [mm]: -21.0


######################################
# Phantom descriptor: 4pt calibration 
######################################

Calib, Number of sources: 4
Calib, Vertical phantom offset [mm]: -1.5
Calib, Axial phantom offset [mm]: -38
Calib, Phantom reversed? (no=0/yes=1): 0

Calib 1, Y position [mm]: 14
Calib 1, Z position [mm]: 16
Calib 2, Y position [mm]: 16
Calib 2, Z position [mm]: 7
Calib 3, Y position [mm]: -16
Calib 3, Z position [mm]: -7
Calib 4, Y position [mm]: -11
Calib 4, Z position [mm]: -16


#####################################
# Transformation for SPECT/CT fusion
#####################################

Fusion, Scaling factor: 1

Fusion, Rot 1 about Z axis [deg]: 0
Fusion, Rot 2 about X axis [deg]: 0
Fusion, Rot 3 about Z axis [deg]: 0

Fusion, Transl along X axis [mm]: 0
Fusion, Transl along Y axis [mm]: 0
Fusion, Transl along Z axis [mm]: 0


#############################
# Positioning of 4pt phantom
#############################

Calib, Rot 1 about Z axis [deg]: 0
Calib, Rot 2 about X axis [deg]: 0
Calib, Rot 3 about Z axis [deg]: 0

Calib, Transl along X axis [mm]: 0
Calib, Transl along Y axis [mm]: 0
Calib, Transl along Z axis [mm]: 0

######################################
